Question 1. It is compatible with DC motors or bipolar step motor

Question 2. The maximum number of independently controlled motor is 2

Question 3. Its 250 mohm to 160 mohms

Question 4. We are using PMOD PORTA on FPGA, which correspond to J1 on the schemetic