Question 1. It is compatible with DC motors

Question 2. The maximum number of independently controlled motor is 2

Question 3. The I/O pins generally have 200-ohm resistor for ESD and short circuit protection

Question 4. We are using USER EXPANSION PORT JP2 (3.3V) to control the motor.