Question 1. With USB 3.0 devices, 300MB/s

Question 2. CVM300-D[9:0] is the data signal, that parallelly output 10 bits of pixel data, Line Valid signal goes high during the readout of each line of pixels within a frame and data valid signal is asserted during each valid pixel output within a line, synchronizing data with clock

Question 3.