1. The Resistance is 47 ohms with 0.02% tolerance
2. P=V^2/R = 0.5W, solve for we have Vmax = 4.85V