Question 1.

We have 32 WireIn and WireOut each

Question 2.

For USB 3.0 we have data depth for wire is 32

Question 3.

Assuming EP\_READY is always on (maximum data throughput) the maximum data bandwidth would be 100.8MHz \* 32bit/8 = 403.2Mb/s

Question 4.

